{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"1","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"merged":[[0,0,0,7],[2,1,2,7],[8,1,8,7],[40,0,40,6]],"flags":["formulas_cached_only"]}
["广东省社会福利服务中心二期建设配套项目（标识导引系统）需求明细清单\n（仅供参考）"]
["序号","项  目","规格","材料/工艺","数量","单位","单价","合计"]
["一","户外一级导视"]
[1,"主楼楼顶发光字","W2000mm*H3000mm*11个字","1、材料：1.0mm镀锌铁皮板、镀锌角钢、LED灯珠；2、工艺：切割、焊接、数控冲孔，灯距30 mm横竖直线均匀，喷氟碳底漆字面再烤2k汽车漆；3、固定：焊成平面边厚100 mm，平字底用30mm*30mm*3mm镀锌角钢连接加固；4、发光字：字样尺寸：W2500mm*H3300mm*9个字；5、光源：48V9 mm红色LED灯粒，48V防水型变压器，配备定时开启的配电箱一套。",1,"套"]
[2,"主楼外墙广告字","W2500mm*H2500mm*1Logo\n+W2300mm*H2300mm*11字","1、材质：1.0mm镀锌铁皮板、LED灯珠。2、工艺：切割、焊接、数控冲孔，灯距30 mm横竖直线均匀，喷氟碳底漆字面再烤2k汽车漆。3、固定：外墙发光字用不锈钢自攻螺丝固定。4、发光字字样尺寸：不锈钢氩孤焊成平面，边厚50mm，喷氟碳底漆再烤面漆。5、光源：48V9 mm红色LED灯粒，48V防水型变压器，配备定时开启的配电箱一套。",1,"套"]
[3,"主楼大门入口发光字","W1500mm*H1500mm*1Logo\nW1200mm*H1200mm*3字","1、材质：0.8mm304不锈钢板、不锈钢方管、LED灯珠。2、工艺：切割、焊接、数控冲孔，灯距30 mm横竖直线均匀，喷氟碳底漆字面再烤2k汽车漆。3、固定：发光字焊接于支撑架上面固定。4、颐养楼和LOGO发光字字样尺寸：0.8mm厚 304不锈钢氩孤焊成支撑架，边厚50mm，喷氟碳底漆再烤面漆。5、光源：48V9 mm红色LED灯粒，48V防水型变压器，配备定时开启的配电箱一套。",1,"套"]
[4,"主楼楼顶钢架","H3000mm*L26500mm","1、材质：全部镀锌角钢；2、工艺：切割、焊接。3、固定：镀锌角钢架用50mm*50mm，40mm*40mm*12mm厚国标方管连接焊成5000mm高25000mm长。200mm*200mm，20mm厚钢板加植根丝固定底座。",1,"套"]
[5,"停车场指引立牌","W700mm*H2200mm*L150mm","1、材质：铝合金型材、双面铝板。2、工艺：铝合金型材边框油漆烤涂，双面铝板专用油漆烤涂底漆面漆内容专用油墨丝印，内置龙骨钢架支撑。3、固定：混凝土浇注基座底脚，钢架埋地安装。",1,"个"]
["二","单元楼标识导向牌"]
[1,"无障碍通道","H330mm*W330mm*5个中文字及英文","1、材质：PVC板。2、工艺：精工切割，表面油漆喷漆。3、固定：玻璃胶+易溶胶粘贴。4、尺寸：10mm厚PVC板。",5,"个"]
[2,"专家介绍栏、宣传栏","W4000*H1500mm","1、材质：铝合金框、PVC板；2、工艺：切割成型、喷画；3、固定：自攻螺丝或免钉胶固定；4、海报夹，框40mm，厚25mm,铝合金边框+PVC+喷画；5、带楣额。",3,"个"]
[3,"宣传栏","W2000mm*H1200mm","1、材质：铝合金框、PVC板；2、工艺：切割成型、喷画；3、固定：自攻螺丝或免钉胶固定；4、海报夹，框40mm，厚25mm,铝合金边框+PVC+喷画",10,"个"]
[4,"科室功能与人员情况介绍栏","W2000mm*H1200mm","1、材质：铝合金框、PVC板；2、工艺：切割成型、喷画；3、固定：自攻螺丝或免钉胶固定；4、海报夹，框40mm，厚25mm,铝合金边框+PVC+喷画",8,"个"]
[5,"护士站","H370mm*W130mm","1、材质：亚克力；2、工艺：热弯工艺、丝印；3、固定：自攻螺丝或免钉胶侧挂安装",7,"个"]
[6,"电梯指示牌","H370mm*W130mm","1、材质：亚克力；2、工艺：热弯工艺、丝印；3、固定：自攻螺丝或免钉胶侧挂安装",8,"个"]
[7,"步梯指示牌","H370mm*W130mm","1、材质：亚克力；2、工艺：热弯工艺、丝印；3、固定：自攻螺丝或免钉胶侧挂安装",16,"个"]
[8,"电梯号码牌①号梯、②号梯、污梯","Φ150mm","1、材质：PVC板。2、工艺：精工切割、喷哑光漆。3、固定：玻璃胶+易溶胶粘贴；4、尺寸：8mm厚。",8,"个"]
[9,"步梯（楼层号码牌）","Φ300mm","1、材质：亚克力板、PVC板；2、工艺：精工切割，表面专用油漆喷漆颜色内容专用油墨丝印；3、固定：玻璃胶+易溶胶粘贴；4、尺寸：5mm厚。",16,"个"]
[10,"电梯（楼层号码牌）","Φ300mm,300mm*300mm","1、材质：亚克力板；2、工艺：精工切割，表面专用油漆喷漆颜色内容专用油墨丝印；3、固定：玻璃胶+易溶胶粘贴；4、尺寸：5mm厚。",8,"个"]
[11,"房间内消防图（无科室名）","300mm*210mm","1、材质：亚克力板；2、工艺：精工切割，表面专用油漆喷漆颜色内容专用油墨丝印；3、固定：玻璃胶+易溶胶粘贴；4、尺寸：5mm厚。",200,"个"]
[12,"走廊消防图（有科室名）","550mm*390mm","1、材质：亚克力板；2、工艺：精工切割，表面专用油漆喷漆颜色内容专用油墨丝印，热弯工艺；3、固定：玻璃胶+易溶胶粘贴；4、尺寸：5mm厚。",50,"个"]
[13,"温馨提示牌（禁止吸烟）","禁止吸烟：W300mm*H150mm","1、材质：亚克力板；2、工艺：精工切割，表面专用油漆喷漆颜色内容专用油墨丝印；3、固定：玻璃胶+易溶胶粘贴；4、尺寸：5mm厚。",300,"个"]
[14,"温馨提示牌（静字）","静字：Φ350mm","1、材质：亚克力板；2、工艺：精工切割，表面专用油漆喷漆颜色内容专用油墨丝印；3、固定：玻璃胶+易溶胶粘贴；4、尺寸：5mm厚。",50,"个"]
[15,"步梯内楼层分流牌","W550mm*390mm","1、材质：铝合金型材；2、工艺：油漆烤涂，专用油墨丝印；3、固定：ABS扣件固定；",34,"个"]
[16,"步梯内消防图","550mm*390mm","1、材质：亚克力板；2、工艺：精工切割，表面专用油漆喷漆颜色内容专用油墨丝印，热弯工艺；3、固定：玻璃胶+易溶胶粘贴；4、尺寸：5mm厚。",34,"个"]
[17,"洗手间牌","H370mm*W130mm","1、材质：亚克力；2、工艺：精工切割，表面专用油漆喷漆颜色内容专用油墨丝印丝印，热弯工艺；3、固定：自攻螺丝或免钉胶侧挂安装",20,"个"]
[18,"床尾信息牌","W210mm*H150mm","1、材质：铝合金型材；2、工艺：、工艺：精工切割，表面专用油漆喷漆颜色内容专用油墨丝印丝印；3、固定: 玻璃胶+易溶胶粘贴；4、尺寸：5mm厚。",200,"个"]
[19,"科室分类牌(横牌)","W330mm*H150mm","1、材质：亚克力板；2、工艺：精工切割、油墨丝印，热弯工艺；3、固定: 玻璃胶+易溶胶粘贴；4、尺寸：5mm厚，5mm+5mm双层。",10,"个"]
[20,"分流指示牌","550mm*390mm","1、材质：铝合金型材。2、工艺：油漆烤涂，专用油墨丝印。3、固定：ABS扣件固定",50,"个"]
[21,"警示标语","300mm*150mm;","1、材质：亚克力板。2、工艺：精工切割、油墨丝印。3、固定：玻璃胶+易溶胶粘贴；4、尺寸：5mm厚。",30,"个"]
[22,"监控警示标志","W300mm*H150mm","1、材质：亚克力板。2、工艺：精工切割、油墨丝印。3、固定：玻璃胶+易溶胶粘贴；4、尺寸：5mm厚。",102,"个"]
[23,"其它安全提示","W300mm*H150mm","1、材质：亚克力板。2、工艺：精工切割、油墨丝印。3、固定：玻璃胶+易溶胶粘贴；4、尺寸：5mm厚。",200,"个"]
[24,"电梯外索引图","W580mm*H10500mm","1、材质：铝合金型材；2、工艺：、工艺：精工切割，表面专用油漆喷漆颜色内容专用油墨丝印丝印；3、固定：玻璃胶+易溶胶粘贴；4、尺寸：5mm厚。",17,"个"]
[25,"电梯内索引图","W580mm*H1050mm","1、材质：铝合金型材；2、工艺：、工艺：精工切割，表面专用油漆喷漆颜色内容专用油墨丝印丝印；3、固定：玻璃胶+易溶胶粘贴；4、尺寸：5mm厚。",6,"个"]
[26,"科室制度上墙（室外）","W600*H900","1、材质：铝合金边框、PVC底板、喷画；2、工艺：切割成型、海报夹喷画；3、固定：自攻螺丝或免钉胶固定；4、尺寸：框25mm，厚20mm,铝合金边框+PVC+喷画。",20,"个"]
[27,"科室制度上墙（室内可换画）","W500*H800","1、材质：亚克力板、广告钉、喷画；2、工艺：精工切割；3、固定：5mm+5mm亚克力板夹喷画、广告钉固定。",273,"个"]
[28,"门牌号码牌","W150mm*H60mm","1、材质：亚克力板。2、工艺：精工切割、油墨丝印。3、固定：玻璃胶+易溶胶粘贴；4、尺寸：5mm厚。",200,"个"]
[29,"护士站水晶字（加英文、面板烤漆）","300mm*300mm","1、材质：水晶板、亚克力板。2、工艺：精工切割、面板烤漆、粘贴。3、固定：玻璃胶+易溶胶粘贴固定。",7,"个"]
[30,"科室分类牌(三角牌)","370mm*130mm","1、材质：亚克力；2、工艺：热弯工艺、丝印；3、固定：自攻螺丝或免钉胶侧挂安装",100,"个"]
[31,"科室分类牌（贴墙牌）","300mm*150mm","1、材质：亚克力板。2、工艺：精工切割、油墨丝印。3、固定：玻璃胶+易溶胶粘贴；4、尺寸：5mm厚。",12,"个"]
["概算合计"]