{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":14,"n_cols":7,"rows_kept":14,"merged":[[1,0,1,6],[13,0,13,6]],"flags":["formulas_cached_only"]}
["附件："]
["零星基建日常工程施工项目清单"]
["序号","项目名称","项目特征描述","计量单位","暂定工程量","综合单价","综合合价"]
[1,"新做木纹色铝合金门","1.门代号及洞口尺寸:木纹色铝合金单开门；\n2.门框或扇外围尺寸:1100mm×2100mm；\n3.其他:不锈钢拉手、门锁等五金配件综合考虑，符合其他设计要求；\n4.其他:综合考虑相关配件和工艺措施。","樘",1]
[2,"新做木质门","1.门代号及洞口尺寸:木饰面单开门；\n2.门框或扇外围尺寸:1100mm×2100mm；\n3.其他:不锈钢拉手、门锁等五金配件综合考虑，符合其他设计要求；\n4.其他:综合考虑相关配件和工艺措施。","樘",1]
[3,"新装铝扣板天花","1.龙骨材料种类、规格、中距:U型轻钢龙骨（不上人）；\n2.面层材料品种、规格:600×600铝扣板面层；\n3.其他:综合考虑相关配件和工艺措施。","㎡",20]
[4,"墙面一般抹灰","1.工作内容：房间墙面抹灰修补；\n2.抹灰厚度、砂浆强度：20mm厚M20水泥砂浆；\n3.其他:综合考虑相关配件和工艺措施。","㎡",40]
[5,"墙面满刮腻子","1.基层类型:砖墙；\n2.腻子种类:成品腻子膏耐水型（N）；\n3.腻子粉品牌：立邦或德高；\n4.刮腻子遍数:两遍；\n5.其他:综合考虑相关配件和工艺措施。","㎡",40]
[6,"墙面乳胶漆","1.基层类型:一般抹灰面；\n2.油漆品种、刷漆遍数:白色乳胶漆（两底两面）；\n3.油漆品牌:多乐士或立邦；\n4.其他:综合考虑相关配件和工艺措施。","㎡",40]
[7,"新建隔墙","1.骨架、边框材料种类、规格:轻钢龙骨硅酸钙板隔墙；\n2.隔板材料品种、规格、颜色:12mm双面硅酸钙板；\n3.其他:综合考虑相关配件和工艺措施。","㎡",20]
[8,"墙面木饰面板（护墙板）安装","1.基层材料种类、规格：阻燃胶合板，9mm厚；\n2.面层材料品种、规格、颜色:木饰面；\n3.安装方式：胶粘。","㎡",10]
[9,"水泥混凝土路面修补（含开挖及基层）","1.人工或机械开挖，厚度50cm，回填20cm夯实；\n2.基层：碎石粉或C20强度混凝土，厚度10cm；\n3.混凝土强度等级:C30商品混凝土；\n4.厚度:20cm；\n5.养生：水养生；\n6.伸缩缝：沥青玛蹄脂；","㎡",30]
[10,"新铺PVC地胶","1.等级：国产优品；\n2.4.0mm厚卷材，含国产环保胶水满粘，接缝热熔胶缝拼接；\n3.其他:综合考虑相关配件和工艺措施。","㎡",30]
["综合单价及综合合价指含材料、人工及安全文明施工费，各项措施费等，不含税。"]